Optimal VFA yields from poultry manure was achieved at pH 9.5
8 g VS L⁻¹ d⁻¹ was identified as the optimal OLR for continuous VFA production
Sulfate-reducing and hydrolytic bacteria dominated at high OLRs
Poultry manure was demonstrated as a viable substrate for VFA production
