Highlights:
- Hydrothermal carbonization of mixed rice husk and food waste improved hydrochar fuel quality.
- Reaction temperature governed hydrochar yield and energy recovery, while feedstock ratio mainly affected HHV.
- Response surface optimization identified moderate temperature and intermediate blending as optimal HTC conditions.
