Apendix 1
 Measurement model assessment and structural model indicators by subsample
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Note: ED=ecodesign; EF=ecoeffiency; SMM= Sustainable Materials Management; OS= Sustainabilty orientation


