Highlights
 Thermal runaway of 15 Ah LFP batteries is characterized at different rates.
 Multi-parameter monitoring reveals electro-thermo-mechanical-gas coupling during thermal runaway.
 Temperature rise and heat release scale non-linearly with overcharge rates.
 Higher overcharge rates shorten runaway onset and exacerbate hazard severity.

