Supplementary Table Captions and Footnotes
Supplementary Table S1. Distribution of vasoactive drug types and dosages used intraoperatively and postoperatively
Note: Drug use is presented as n (%) and dosage as median [interquartile range]. P values compare the non-AKI and AKI groups. AKI, acute kidney injury.
Supplementary Table S2. Final confounders identified through multivariable analysis for the mediation analyses
Note: Each column presents a multivariable logistic regression model for postoperative AKI with the indicated exposure or mediator included. Odds ratios are reported with 95% confidence intervals. BMI, body mass index; NYHA, New York Heart Association; CPB, cardiopulmonary bypass; PASP, pulmonary artery systolic pressure; MAP_TIME_65, cumulative duration below 65 mmHg; MAP_AUT_65, area under the 65-mmHg threshold; VIS, vasoactive-inotropic score; OR, odds ratio; CI, confidence interval; AKI, acute kidney injury.
Supplementary Table S3. Mediation effects of perioperative hemodynamic changes on the PH-AKI association using causal stepwise regression
Note: Adjusted models included age, sex, BMI, smoking history, hypertension, preoperative serum creatinine, neutrophil count, neutrophil-to-lymphocyte ratio, platelet count, and CPB duration. Path c represents the total effect, path a the exposure-mediator association, path b the mediator-outcome association, c' the direct effect, ab the indirect effect, ab/c' the mediation-to-direct effect ratio, and ab/(ab+c') the proportion mediated. PH, pulmonary hypertension; AKI, acute kidney injury; PASP, pulmonary artery systolic pressure; MAP_TIME_65, cumulative duration below 65 mmHg; MAP_AUT_65, area under the 65-mmHg threshold; VIS, vasoactive-inotropic score.
Supplementary Table S4. Comprehensive diagnostic metrics for ROC-derived thresholds of MAP_TIME_65 and postoperative VIS
Note: Cutoffs were determined by maximizing the Youden index (J = sensitivity + specificity - 1). MAP_TIME_65, cumulative duration below 65 mmHg; VIS, vasoactive-inotropic score; AUROC, area under the receiver operating characteristic curve; ROC, receiver operating characteristic.
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