1. OLAHW and solution treatment yield 2507 SDSS joints with proper phase ratio.
2. Oscillating laser refines HAZ ferrite grains from 26.4 to 13.6 μm.
3. Oscillation shifts fracture to base metal, boosting mechanical properties.
4. Synergy achieves optimal ductility and corrosion resistance in the joints.
