Multidimensional characteristics and ecological risks of MPs in receiving waters from 
WWTP effluent
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Figure. S1 Different shaped particles extracted from the samples（a. fiber; b. film; c. fragment; d. particle）
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Figure. S2 The FTIR spectrum of the main polymers present in the types of MPs
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