        Graphical abstract:
The roughness of metallic nickel and cobalt has been reduced effectively in a suitable electrolytic bath, namely, 1 M ChCl: 2 M Lac. The surface smoothness of metallic nickel and cobalt is 78% and 51%, respectively.
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