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	Figure S1. Water contact angle images of (a) CNT aerogel and (b) Fe₃O₄–CNT magnetic aerogel.
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Figure S2. The UV-Vis spectra (left) and standard diagram (right) for correlation between the adsorption of aniline solutions at 232 nm and their concentrations.
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	Figure S3. UV–Vis absorption spectra for the optimization of catalyst loading.
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	Figure S4. UV–Vis absorption spectra for the optimization of reaction temperature.
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	Figure S5. UV–Vis absorption spectra for the optimization of NaOH amount.
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	Figure S6. UV–Vis absorption spectra for the optimization of reaction time.
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