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Figure S1. 1H NMR of 2a in CDCl3
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Figure S2. 1H NMR of 2b in CDCl3
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Figure S3. 1H NMR of 2c in CDCl3
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Figure S4. DSC of Gel Polymer Electrolyte (entry 1, Table 1)
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Figure S5. DSC of Gel Polymer Electrolyte (entry 2, Table 1)
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Figure S6. DSC of Gel Polymer Electrolyte (entry 3, Table 1)
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Figure S7. DSC of Gel Polymer Electrolyte  (entry 4, Table 1)
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Figure S8. DSC of Gel Polymer Electrolyte (entry 5, Table 1)
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Figure S9. DSC of Gel Polymer Electrolyte (entry 6, Table 1)
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