Supplementary Materials
Supplemental Table S1. The detail of mass spectrometry parameters.

	Description
	Parameters

	Scan type(m/z)
	70-1050

	Sheath gas flow (arb)
	50

	Aux gas flow rate (arb)
	13

	Heater temp (℃)
	425

	Capillary temp (℃)
	325

	Spray voltage (+)(V)
	3500

	Spray voltage (-)(V)
	-3500

	Normalized collision energy(eV)
	20.40.60

	Resolution (Full MS)
	60,000

	Resolution(MS2)
	7500



