EDF-6. Recommended 176Hf/177Hf value for zircon reference materials and weighted mean standard corrected ratio obtained in each analytical session (Mud Tank primary reference material).
	Zircon standard
	Recommended 176Hf/177Hf 
	Weighted mean for session 1 (24/2/2021)
	Weighted mean for session 2 (25/2/2021)
	Weighted mean for session 3 (26/2/2021)

	Mud Tank
	0.282505 ± 0.000044
(Woodhead and Hergt, 2005)
	0.282507 ± 0.000012 
(MSWD = 0.72,
n = 14)
	0.282507 ± 0.000014 (MSWD = 0.29,
n = 16)
	0.282507 ± 0.000015 (MSWD = 0.83,
n = 14

	GJ-1
	0.282000 ± 0.00005, (Morel et al., 2008)
	0.282022 ± 0.000015 (MSWD = 0.68,
n = 14)
	0.282024 ± 0.000018 (MSWD = 0.18,
n = 14)
	0.282024 ± 0.000016 (MSWD = 1.5,
n = 15)

	R33
	0.282764 ± 0.000014
(Fisher et al., 2014)
	0.282743 ± 0.000015 
(MSWD = 0.19,
n = 11)
	0.2824757 ± 0.000016 (MSWD = 1.2,
n = 14)
	0.282758 ± 0.000016 (MSWD = 0.66,
n = 14)

	91500
	0.282306 ± 0.00004
(Woodhead et al., 2004)
	0.282308 ± 0.000018 
(MSWD = 1.2,
n = 15)
	0.282298 ± 0.000021 (MSWD = 0.83,
n = 14)
	0.282310 ± 0.000017 (MSWD = 0.71,
n = 18)



