
EDF-7 Recommended ages for zircon reference materials and weighted mean standard corrected ages obtained in each analytical session.
	Zircon standard
	Recommended age (Ma)
	Weighted mean for session 1 (24/2/2021)
	Weighted mean for session 2 (25/2/2021)
	Weighted mean for session 3 (26/2/2021)

	GJ-1
	608.5 ± 1.5 Ma 
(Jackson et al., 2004)
601.5± 0.40 Ma
(Horstwood et al., 2016)
	605.6 ± 2.2Ma 
(MSWD = 0.18, 
n = 15)
	608.2± 0.93 Ma 
(MSWD = 3.8, 
n = 16)
	

607.3± 1.5 Ma
(MSWD = 0.99,
n = 14)

	Maniitsoq
	3007.3 ± 0.3 Ma
(March et al., 2019)
	3003.8 ± 4.1 Ma 
(MSWD = 3.5, 
n = 9)
	-
	3008.3 ± 7.8 Ma 
(MSWD = 2.1, 
n = 7)


	91500
	1062.4 ± 0.4 Ma
(Wiedenbeck et al., 1995)
	1061.0 ± 4 Ma
(MSWD = 0.61, 
n = 14)
	1062.3 ± 2.2 Ma
(MSWD = 0.05, 
n = 14)
	1062.3 ± 2.6 Ma
(MSWD = 0.53, 
n = 16)

	OGC
	3467 ± 3 Ma
(Stern et al., 2009)
	3465.1 ± 2.9 Ma
(MSWD = 0.48, 
n = 13)
	-
	3464.9 ± 5.1 Ma
(MSWD = 0.66, 
n = 13)

	Note: No grains >1400Ma were measured in session 2 so older standards were not required. 



