· Facile hydrothermal synthesis of Ni–Co–S/MOF @ Functionalized MWCNT composite. 
· High specific capacitance of 820 F.g−1 at 0.5 A.g−1 for the hybrid electrode. 
· Excellent cycling stability with ~93% capacitance retention after 5000 cycles. 
· Symmetric device delivers 41.4 Wh.kg−1 and 720 W.kg−1 (2-electrode setup). 
· Synergistic MOF porosity and CNT network boost ion/electron transport.
