


Mechanical and abrasion behaviour of cement and alkali-activated material mixes based on oil refinery waste catalyst: investigation and semi-empirical predictive models
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