1.A 3D progressive damage model is developed for SBDS joints with hole-edge delamination.
2.Experimental validation shows prediction errors within 10% for all delamination diameters.
3.Parametric studies reveal the effects of delamination location, shape, and orientation.
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