

Supplementary table 1: MRI specified safety conditions for the HiRes™ Ultra 3D CI with a self-aligning diametric magnet, and the subsequent five a HiRes 90K™ CI with an axial magnet at 1.5T


	Implant
	Spatial gradient field (T/m)
	Maximum head SAR (W/kg)
	Maximum body SAR(W/kg)

	HiRes™ Ultra 3D CI
	20
	≤3.2
	≤2

	HiRes 90K™ CI
	2.5
	≤1
	≤1.7







