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Supplementary Bland-Altman Plots for GNSS-RTK vs Reference System

Figure S1: Bland-Altman Plot for Total Distance Figure S2: Bland-Altman Plot for Peak Speed Figure S3: Bland-Altman Plot for LSR Distance
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Figure S4: Bland-Altman Plot for HSR Distance Figure S5: Bland-Altman Plot for VHSR Distance
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