Sonochemical Fabrication of a Stable SERS Platform with Silver Nanoparticles on PCL Nanofibers
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Supplementary Results
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Figure S1. Electroplated film production with Nanospider® system A) Control unit; B) 1) Collector roll (fabric), 2) Polymer solution loading to carrier (polymer resorvir), 3) Polymer resorvier (carrier), 4) Feeding wire(bottom) and solution spraying part, and 5) Nanofibers collection on roll surface; C) Nanofibers formed during operation; D) Nanofiber film (white-curled) collected on the surface of collector roll (fabric, blue).
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