[bookmark: _Ref219277224]Table 1: Outdoor radiofrequency electromagnetic field (RF-EMF) exposure levels (µW/m²) measured at four building orientations around ten schools in Graz, Austria. Measurements were performed using a broadband field meter (NBM 550, Narda) with an isotropic EF-0691 probe. Values are reported as minimum (Min), average (Avg), and maximum (Max) power density.
	School
	Date
	Orientation
	Min (µW/m²)
	Avg (µW/m²)
	Max (µW/m²)

	Mittelschule St. Andrä
	Dec 09, 2025
	North
	<106
	1,962
	7,847

	
	
	East
	1,020
	7,047
	45,903

	
	
	South
	363
	2,008
	15,922

	
	
	West
	586
	4,906
	20,353

	Modellschule Graz
	Dec 09, 2025
	North
	344
	1,453
	6,706

	
	
	East
	468
	3,569
	10,716

	
	
	South
	1,375
	8,786
	29,414

	
	
	West
	289
	1,655
	9,276

	BRG Körösi
	Dec 10, 2025
	North
	<106
	117
	1,053

	
	
	East
	<106
	307
	2,054

	
	
	South
	<106
	255
	1,263

	
	
	West
	<106
	383
	2,008

	BRG Carneri
	Dec 10, 2025
	North
	45
	923
	2,547

	
	
	East
	<106
	923
	6,209

	
	
	South
	403
	2,924
	10,190

	
	
	West
	<106
	446
	2,344

	Praxismittelschule PH Steiermark
	Dec 10, 2025
	North
	1,155
	9,576
	55,640

	
	
	East
	1,300
	8,883
	58,594

	
	
	South
	307
	4,346
	27,162

	
	
	West
	955
	3,631
	25,327

	BRG Lichtenfels
	Dec 11, 2025
	North
	307
	8,594
	33,996

	
	
	East
	1,492
	5,889
	13,428

	
	
	South
	<106
	1,053
	2,760

	
	
	West
	<106
	802
	4,414

	HLW Schrödinger
	Dec 11, 2025
	North
	179
	1,414
	10,610

	
	
	East
	514
	3,037
	17,248

	
	
	South
	<106
	892
	6,622

	
	
	West
	1,300
	12,955
	40,552

	BRG Seebacher
	Dec 11, 2025
	North
	<106
	1,227
	12,955

	
	
	East
	1,698
	6,622
	21,094

	
	
	South
	2,760
	14,524
	47,911

	
	
	West
	<106
	446
	5,889

	VS St. Leonhard
	Dec 11, 2025
	North
	60
	1,121
	3,387

	
	
	East
	<106
	773
	10,823

	
	
	South
	955
	9,276
	27,845

	
	
	West
	<106
	2,101
	10,823

	BRG Klusemannstraße
	Dec 11, 2025
	North
	<106
	1,492
	18,069

	
	
	East
	10
	923
	21,094

	
	
	South
	<106
	1,655
	23,873

	
	
	West
	166
	2,008
	9,475



