Supplementary Table S1. MRI acquisition parameters.
	MRI acquisition parameters

	MRI system
	3.0-T Siemens Prisma (Erlangen, Germany)

	Receive coil
	64-channel head/neck coil

	Resting-state fMRI

	Sequence
	Blood oxygen level-dependent gradient-echo echo-planar imaging (EPI)

	Repetition time (TR)
	2,000 ms

	Echo time (TE)
	30 ms

	Matrix
	64 × 64

	Field of view (FOV)
	230 × 230 mm²

	Flip angle
	90°

	Slice number
	37

	Slice thickness
	3.6 mm

	Slice gap
	0.36 mm

	Acquired voxel size
	3.6 × 3.6 × 3.6 mm³

	Diffusion MRI

	Sequence
	Diffusion tensor imaging echo-planar imaging (EPI)

	Repetition time (TR)
	5,000 ms

	Echo time (TE)
	69 ms

	Matrix
	128 × 128

	Field of view (FOV)
	224 × 224 mm²

	Flip angle
	90°

	Slice number
	35

	Slice thickness
	3.5 mm

	Slice gap
	0.70 mm

	Acquired voxel size
	1.75 × 1.75 × 3.5 mm³

	b values
	0 and 1,000 s/mm²

	Diffusion-weighted volumes
	90 at b = 1,000 s/mm²

	b0 volumes
	12

	Structural MRI

	Sequence
	Three-dimensional T1-weighted magnetization-prepared rapid gradient-echo (MPRAGE)

	Repetition time (TR)
	2,200 ms

	Echo time (TE)
	2.48 ms

	Inversion time (TI)
	900 ms

	Matrix
	256 × 256

	Field of view (FOV)
	230 × 230 mm²

	Flip angle
	8°

	Slice thickness
	1.0 mm

	Voxel size
	0.9 × 0.9 × 1.0 mm³


