Table 5. Urodynamic parameters at baseline and after treatment, as well as changes in parameters between patients with and without successful treatment outcomes
	Urodynamic parameters
	GRA ≥ 2 (n=163)
	GRA < 2 (n=49)
	p-value

	FSF (ml)
	Baseline
	185.4±100.2
	175.9±93.5
	

	
	Follow up
	162.4±77.2
	186.0±100.2
	

	
	Δ change
	-23.0±109.3
	10.1±94.7
	0.115

	FS (ml)
	Baseline
	285.3±123.1
	278.8±129.5
	

	
	Follow up
	269.8±116.7
	284.4±116.8
	

	
	Δ change
	-15.5±135.0
	5.6±137.0
	0.434

	US (ml)
	Baseline
	326.1±131.0
	332.4±135.8
	

	
	Follow up
	307.6±126.0
	327.9±123.4
	

	
	Δ change
	-18.6±140.3
	-4.5±151.1
	0.621

	Compliance
	Baseline
	67.7±85.7
	65.6±52.0
	

	
	Follow up
	73.2±87.5
	83.5±85.8
	

	
	Δ change
	5.6±92.3
	17.9±102.7
	0.518

	Pves (cmH2O)

	Baseline
	52.4±41.9
	57.4±42.5
	

	
	Follow up
	50.8±32.4
	64.7±38.5
	

	
	Δ change
	-1.6±42.4
	7.3±45.5
	0.306

	Pdet (cmH2O)
	Baseline
	8.1±10.5
	9.5±10.6
	

	
	Follow up
	9.5±13.2
	12.1±22.3
	

	
	Δ change
	1.3±14.8
	2.6±23.2
	0.712

	Qmax (ml/s)
	Baseline
	3.8±4.9
	2.9±5.3
	

	
	Follow up
	11.4±8.8
	6.1±9.5
	

	
	Δ change
	7.6±9.4*
	3.2±7.7
	0.007*

	PVR (ml)
	Baseline
	328.7±194.7
	417.4±201.6
	

	
	Follow up
	98.9±125.8
	309.5±231.6
	

	
	Δ change
	-229.8±220.8*
	-107.9±245.3
	0.002*

	CBC (ml)
	Baseline
	412.3±179.2
	477.8±187.9
	

	
	Follow up
	298.0±155.9
	412.0±207.1
	

	
	Δ change
	-114.3±212.9-*
	-65.8±256.3
	0.227

	VE
	Baseline
	0.22±0.28
	0.11±0.22
	

	
	Follow up
	0.69±0.30
	0.28±0.32
	

	
	Δ change
	0.58±0.37*
	0.17±0.28
	<0.001*

	BOOI
	Baseline
	1.3±12.3
	3.3±14.8
	

	
	Follow up
	-9.1±17.2
	1.0±28.5
	

	
	Δ change
	-10.4±17.8*
	-2.4±25.3
	0.049*

	BCI
	Baseline
	25.5±28.6
	24.9±30.6
	

	
	Follow up
	56.2±36.0
	40.0±50.9
	

	
	Δ change
	30.7±43.7*
	15.1±44.7
	0.077


GRA: global response assessment, FSF: first sensation of filling, FS: full sensation, US: urge sensation, Pves: intravesical pressure, Pdet: detrusor pressure, Qmax: maximum flow rate, PVR: post-void residual, CBC: cystometric bladder capacity, VE: voiding efficiency, BOOI: bladder outlet obstruction index, BCL bladder contractility index

