TABLES
Table 1. Relative weights for GWQI calculation
	
pH
	6.5–8.5
	4
	0.105

	EC (µS/cm)
	1500
	4
	0.105

	TH (°F)
	30
	2
	0.053

	Ca²⁺ (mg/L)
	200
	2
	0.053

	Mg²⁺ (mg/L)
	150
	2
	0.053

	Cl⁻ (mg/L)
	250
	3
	0.079

	SO₄²⁻ (mg/L)
	250
	4
	0.105

	HCO₃⁻ (mg/L)
	1000
	3
	0.079

	NO₃⁻ (mg/L)
	50
	5
	0.132

	NH₄⁺ (mg/L)
	0.5
	3
	0.079
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Descriptive Statistics of Groundwater Quality Parameters
F'kirina Region, 2018-2021

arameter Mean std Min Max WHO Standard
pH 7.37 0.24 7.08 7.58 6.5-8.5
EC (uSfcm) 1096.90 298.21 609.50 1359.50 1500
Turbidity (NTU) 4.01 5.31 0.21 12.90 1
TH (°F) 43.80 11.23 26.25 56.00 30
ca’' (mgfL) 129.60 48.12 63.00 190.50 200
Mg’ {mg/L) 2935 6.24 20.25 37.75 150
al (mgiL) 149.90 63.47 5450 227.00 250
504 (mg/L) 7275 48.76 0.00 134.00 250
HCOs (mg/L) 294.10 158.90 136.25 533.75 1000
NO: {mg/L) 33.95 1195 19.00 49.75 50
NHa ' (mg/L) 0.03 0.02 0.01 0.06 05
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Groundwater Quality Index (GWQI) Assessment Results
F'kirina Region, Oum El Bouaghi, Algeria

Borehole GWQI Value Quality Class
137 63.51 Poor Unsuitable for drinking without treatment
oL1 64.56 Poor Unsuitable for drinking without treatment
045 33.34 Good Suitable for drinking
H47 50.78 Good Suitable for drinking
140 64.68 Poor Unsuitable for drinking without treatment





