
· ML-guided PBF-LB/M enabled M2 HSS processing without baseplate preheating.
· Hatch spacing was identified as the dominant PBF-LB/M process parameter.
· A 60 µm hatch spacing enhanced densification and suppressed delamination.
· [bookmark: _GoBack]EBSD revealed a refined lath structure with strong crystallographic texture.
