
	
Table 1. Physical and chemical properties of the soil (0–30 cm depth) at the Feridounshahr experimental site, Iran.

	Property
	2022–2023
	2023–2024
	2024–2025
	Unit

	Texture
	Clay loam
	Clay loam
	Clay loam
	–

	pH (1:2.5 soil: water)
	7.8
	7.9
	7.7
	–

	Electrical conductivity
	0.65
	0.64
	0.61
	dS m⁻¹

	Organic carbon
	0.82
	0.85
	0.91
	%

	Total nitrogen
	0.05
	0.07
	0.11
	%

	Available P (Olsen)
	12.5
	11.8
	11.8
	mg kg⁻¹

	Available K (NH₄OAc)
	180
	175
	175
	mg kg⁻¹

	Bulk density
	1.35
	1.37
	1.37
	g cm⁻³

	Field capacity
	27.3
	27.3
	27.3
	%
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  Table 1.  Physical and chemical properties of the soil (0 – 30 cm depth) at the  Feridounshahr experimental site, Iran.  

Property  2022 – 2023  2023 – 2024  2024 – 2025  Unit  

Texture  Clay loam  Clay loam  Clay  loam  –  

pH (1:2.5 soil: water)  7.8  7.9  7.7  –  

Electrical  conductivity  0.65  0.64  0.61  dS m ? ¹  

Organic carbon  0.82  0.85  0.91  %  

Total nitrogen  0.05  0.07  0.11  %  

Available P (Olsen)  12.5  11.8  11.8  mg  kg ? ¹  

Available K (NH 4 OAc)  180  175  175  mg  kg ? ¹  

Bulk density  1.35  1.37  1.37  g cm ? ³  

Field capacity  27.3  27.3  27.3  %  

                                 

