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1） Ra6.3  And  Ra3.2

2) The results demonstrate that the stress increases a lot when the bolt is surface rough, whose stress is 11.5% higher than the flat condition. The temperature of Ra6.3 is about 100 degrees higher than the flat condition. It plays a crucial role in enhancing the service life of friction surfaces.
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