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Physics-informed multiscale modeling of high-bandwidth electrohydraulic actuation
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@ Multiscale physics coupling = predictive design + reliable digital twins




