   Table 1 Resistivity and Lithounits.
	Serial No.
	Resistivity (Ω-m)
	Inferred Lithounits

	1
	0-10
	Clay

	2
	10-50
	Cobbles, pebbles, gravel, sand, and clay

	3
	50-100
	Gravels and sand with a thin clay layer 

	4
	100-200
	Cobbles, pebbles, and sandy clay 

	5
	200-300
	Sandy clay with cobbles, pebbles, and gravels 

	6
	300-400
	Boulders, pebbles, and sandy clay 

	7
	>500
	Dry boulder formation with clay 



