
Highlights

(1) EBR at 5 DAA restores leaf function, increasing wheat yield by 12.5% under heat stress.
(2) Maximum grain-filling rate is the key yield determinant under heat stress.
(3) [bookmark: _GoBack]Optimized EBR timing coordinates source–sink relations to mitigate yield loss.
