Appendix A
Table A1 presents the full sensitivity analysis used to evaluate the ΔNDVI threshold and sequential terrain-based filtering parameters applied during development of the landslide mapping workflow.

Table A1 Sensitivity analysis of ΔNDVI thresholds and sequential terrain-based filtering parameters evaluated during development of the landslide mapping workflow.
	Filtering stage
	Scenario / threshold
	No. of polygons
	Total area (km²)
	Area metric (%)
	Decision

	ΔNDVI threshold
	< −0.05
	329,844
	189.71
	10.14
	Not selected – too permissive

	
	< −0.10
	124,932
	72.97
	3.90
	Selected

	
	< −0.15
	46,542
	29.20
	1.56
	Not selected – more restrictive

	
	< −0.20
	19,808
	12.74
	0.68
	Not selected – more restrictive

	
	< −0.25
	9,778
	5.36
	0.29
	Not selected – removed true landslides

	River buffer
	0 m
	124,932
	72.97
	0.00
	Baseline

	
	25 m
	117,354
	66.02
	9.52
	Not selected – limited filtering

	
	50 m
	110,965
	62.51
	14.34
	Selected

	
	75 m
	106,518
	59.49
	18.48
	Not selected – more restrictive

	
	100 m
	102,955
	56.79
	22.18
	Not selected – removed true landslides

	Elevation filter
	>0 m
	110,965
	62.51
	0.00
	Baseline

	
	>25 m
	99,592
	46.35
	25.85
	Not selected – limited filtering

	
	>50 m
	88,475
	37.66
	39.80
	Not selected – limited filtering

	
	>75 m
	77,961
	31.07
	50.30
	Not selected – limited filtering

	
	>100 m
	66,731
	25.31
	59.50
	Selected

	
	>125 m
	55,650
	19.92
	68.13
	Not selected – removed true landslides

	Slope filter
	River50 + Elev100
	66,731
	25.31
	0.00
	Baseline

	
	Slope >2°
	66,178
	23.89
	5.61
	Not selected – limited filtering

	
	Slope >5°
	63,086
	20.76
	17.98
	Selected

	
	Slope >7.5°
	58,442
	17.31
	31.61
	Not selected – more restrictive

	
	Slope >10°
	52,372
	13.75
	45.67
	Not selected – removed true landslides

	Minimum mapping
unit (MMU)
	200 m²
	18,202
	16.12
	22.35
	Not selected – initial removal of many small, isolated patches

	
	400 m²
	7,510
	13.31
	35.89
	Not selected – high number of small, isolated features remained

	
	500 m²
	5,739
	12.53
	39.64
	Not selected – initial improvement removing small features

	
	600 m²
	4,597
	11.91
	42.63
	Selected

	
	800 m²
	3,219
	10.97
	47.16
	Not selected – removed true landslides

	Manual validation
	Before manual validation (MMU ≥600 m²)
	4,597
	11.91
	—
	Baseline

	
	Final inventory after manual validation
	3,689
	6.91
	42.00
	Final inventory



Note: For the ΔNDVI threshold analysis, area metric represents mapped area relative to the study area. For subsequent filtering stages, it represents area reduction relative to the baseline of each stage.

