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Fig. S1. Calibration curve between NaCl concentration and conductivity.
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Fig. S2. EIS curves of three different current collectors at a flow-electrode rate of 20 mL min-1 and a Bi@NSC concentration of 5 wt%.
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WSC 20.1 1.23


