Highlights
· KOH-activated porous biochar was produced from five waste raw materials.
· Sheet and splash erosions were significantly reduced with increasing biochar rates.
· The type of raw material affected the erosion control efficiency.
· Porous biochar reduced the slope sensitivity of soil detachment due to rainfall.
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