Graphical Abstract
A green rosemary-mediated Ag/Co/La2O3/chitosan nanocomposite was developed with enhanced multifunctional properties. It efficiently removed binary MB/CV (97.5%/94.0%) and retained high activity after seven cycles with limited metal release. The work demonstrates its potential as a sustainable and reusable material for integrated wastewater treatment and antibacterial applications.
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