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Figure S1. Linear plots of the current-density difference (ΔJ) versus scan rate for NF, Ni-MOF/NF, and Fe₃O@Ni-MOF/NF.
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Figure S2. Raw data for the constant current mode of DC-Power supply using two electrode Fe3O4@Ni-MOF/NF at different current ranges. 
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