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S1: Supplementary figures of the displacement validation 
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S2: Supplementary figures of the nominal strain validation 
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