Highlights
· Shallow bitumen seeps are geogenic sources of soil and groundwater contamination.
· Combined numerical and field resistivity studies was used to delineate bitumen seeps
· Prior 1D resistivity data provided prior data for forward modeling study
· Forward modeling results show possible limitations in isolating the bitumen seeps
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