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Summary of the estimated electrical resistivity, layer thickness, curve types and lithological interpretations from the 13 VES Stations
	VES No
	Coordinates
	Elevation (m)
	Layer Resistivity(Ωm)
	Thickness(m)
	Depth(m)
	Probable Lithology
	Curve Type
	RMS Error%

	1
	 6°27'12.67"
	008
	5,231
	0.759
	0.0
	Top Soil
	QH
	5.3

	
	 4°25'16.78"
	
	781
	5.070
	0.759
	Unsaturated-Sand
	 _
	

	
	
	
	102
	7.560
	5.830
	Sand Aquifer
	 _
	

	
	
	
	5,926
	
	13.390
	Bitumen Bearing Bed
	
	

	
	
	
	
	
	
	
	
	

	2
	 6°27'11.90"
	008
	8,301
	0.888
	0
	Top Soil
	QH
	6.0

	
	 4°25'16.58"
	
	2,438
	3.380
	0.888
	Unsaturated-Sand
	 _
	

	
	
	
	739
	5.860
	4.270
	Contaminated Sand Aquifer
	 _
	

	
	
	
	62,332
	
	10.130
	Bitumen Bearing Bed
	
	

	
	
	
	
	
	
	
	
	

	3
	 6°27'12.09"
	007
	6,187
	1.130
	0
	Top Soil
	
KH
	2.6

	
	 4°25'14.99"
	
	12,223
	2.730
	1.130
	Unsaturated-Sand
	 _
	

	
	
	
	4,026
	5.460
	3.860
	Contaminated Sand Aquifer
	 _
	

	
	
	
	353,312
	
	9.330
	Bitumen Bearing Bed
	
	

	
	
	
	
	
	
	
	
	

	4
	 6°27'12.97"
	007
	15,772
	0.512
	0
	Top Soil
	QH
	4.8

	
	 4°25'15.19"
	
	1,268
	6.150
	0.512
	Unsaturated-Sand
	 _
	

	
	
	
	142
	8.470
	6.660
	Sand Aquifer
	 _
	

	
	
	
	5,476
	
	15.130
	Bitumen Bearing Bed
	
	

	
	
	
	
	
	
	
	
	

	5
	60 27’ 15.1’’
	006
	1,167
	2.230
	0
	Top Soil
	KQH
	1.7

	
	40 25’ 15.0’’
	
	2,688
	2.030
	2.230
	Unsaturated Sand
	 _
	

	
	
	
	380
	5.790
	4.270
	Contaminated Sand Aquifer
	 _
	

	
	
	
	53
	11.190
	10.060
	Clean Sand Aquifer
	
	

	
	
	
	402
	
	21.250
	Clayey-Sand
	
	

	
	
	
	
	
	
	
	
	

	6
	60 27’ 13.1’’
	006
	1,720
	0.377
	0
	Top Soil
	KQH
	1.9

	
	40 25’ 14.6’’
	
	9,004
	0.728
	0.377
	Unsaturated Sand
	 _
	

	
	
	
	984
	7.830
	1.110
	Contaminated Sand Aquifer
	_
	

	
	
	
	40
	6.990
	8.940
	Clean Sand Aquifer
	
	

	
	
	
	263
	
	15.930
	Clayey-Sand
	
	

	
	
	
	
	
	
	
	
	

	7
	60 27’ 10.9’’
	007
	20,524
	0.899
	0
	Top Soil
	QQH
	2.7

	
	40 25’ 14.2’’
	
	7,230
	1.990
	0.899
	Unsaturated Sand
	 _
	

	
	
	
	563
	8.830
	2.890
	Contaminated Sand Aquifer
	 _
	

	
	
	
	235
	10.370
	11.720
	Sand Aquifer
	
	

	
	
	
	16,748
	
	22.090
	Bitumen Bearing Bed
	
	

	
	
	
	
	
	
	
	
	

	8
	60 27’ 11.0’’
	007
	25,501
	1.440
	0
	Top Soil
	QHK
	1.8

	
	40 25’ 12.6’’
	
	5,119
	0.919
	1.440
	Unsaturated Sand
	_
	

	
	
	
	315
	4.430
	2.360
	Contaminated Sand Aquifer
	_
	

	
	
	
	3,052
	7.350
	6.790
	Bitumen Bearing Bed
	
	

	
	
	
	547
	
	14.140
	Clayey-Sand
	
	

	
	
	
	
	
	
	
	
	

	9
	60 27’ 13.4’’
	007
	853
	0.454
	0
	Top Soil
	KQH
	1.9

	
	40 25’ 13.0’’
	
	2,498
	0.945
	0.454
	Unsaturated Sand
	 _
	

	
	
	
	903
	6.830
	1.400
	Contaminated Sand Aquifer
	 _
	

	
	
	
	54
	7.740
	8.220
	Clean Sand Aquifer
	
	

	
	
	
	250
	
	15.960
	Clayey-Sand
	
	

	
	
	
	
	
	
	
	
	

	10
	60 27’ 15.5’’
	006
	1,755
	0.374
	0
	Top Soil
	QQH
	2.9

	
	40 25’ 13.5’’
	
	1,469
	5.930
	0.374
	Unsaturated Sand
	 _
	

	
	
	
	248
	9.740
	6.300
	Contaminated Sand Aquifer
	 _
	

	
	
	
	49
	11.990
	16.040
	Clean Sand Aquifer
	
	

	
	
	
	398
	
	28.030
	Clayey-Sand
	
	

	
	
	
	
	
	
	
	
	

	11
	60 27’ 15.9’’
	009
	2,368
	1.600
	0
	Top Soil
	QH
	1.7

	
	40 25’ 11.8’’
	
	1,286
	6.660
	1.600
	Contaminated Sand Aquifer
	 _
	

	
	
	
	32
	6.170
	8.260
	Clean Sand Aquifer
	 _
	

	
	
	
	263
	
	14.420
	Clayey-Sand
	
	

	
	
	
	
	
	
	
	
	

	12
	60 27’ 13.7’’
	008
	1,523
	5.710
	0
	Top Soil
	QH
	1.9

	
	40 25’ 11.4’’
	
	215
	8.800
	5.710
	Contaminated Sand Aquifer
	 _
	

	
	
	
	40
	10.370
	14.500
	Clean Sand Aquifer
	 _
	

	
	
	
	1,083
	
	24.870
	Bitumen Bearing Bed
	
	

	
	
	
	
	
	
	
	
	

	13
	60 27’ 11.9’’
	007
	1,749
	0.580
	0
	Top Soil
	KH
	5.8

	
	40 25’ 11.1’’
	
	4,611
	1.190
	0.580
	Unsaturated Sand
	 _
	

	
	
	
	80
	4.950
	1.770
	Clean Sand Aquifer
	 _
	

	
	
	
	20,769
	
	6.720
	Bitumen Bearing Bed
	
	







Appendix B 
Inverted vertical electrical sounding curves and lithological interpretations
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