A                                 B


 
C                                  D


 
Supplemental_Fig_S4. Real-time G4-ThT-NASBA system detects CSFV fluorescence curve under different ThT concentrations. A: The final concentration of ThT is 2 μM; B: the final concentration of ThT is 4 μM; C: the final concentration of ThT is 6 μM; D: the final concentration of ThT is 8 μM.
image3.emf
0 20 40 60 80 100 120

0

2

4

6

8

10

12

ThT6μM

Time(min)

F

l

u

o

r

e

s

c

e

n

c

e

 

I

n

t

e

n

s

i

t

y

(

a

r

b

.

u

n

i

t

)

Positive

Negative



image4.emf
0 20 40 60 80 100 120

0

2

4

6

8

10

12

ThT8μM

Time(min)

F

l

u

o

r

e

s

c

e

n

c

e

 

I

n

t

e

n

s

i

t

y

(

a

r

b

.

u

n

i

t

)

Positive

Negative



image1.emf
0 20 40 60 80 100 120

0

2

4

6

8

ThT2μM

Time(min)

F

l

u

o

r

e

s

c

e

n

c

e

 

I

n

t

e

n

s

i

t

y

(

a

r

b

.

u

n

i

t

)

Positive

Negative



image2.emf
0 20 40 60 80 100 120

0

2

4

6

8

10

ThT4μM

Time(min)

F

l

u

o

r

e

s

c

e

n

c

e

 

I

n

t

e

n

s

i

t

y

(

a

r

b

.

u

n

i

t

)

Positive

Negative



