Highlights
1. The wood-based composites via heat treatment with high electromagnetic shielding were prepared.
[bookmark: _GoBack]2. The contact angle, thickness and conductivity of composite materials can be up to 120.2°, 100.86 μm and 527 S/cm, respectively.
3. The average electromagnetic shielding efficiency can reach 91.40 dB.

