Highlights
· Soya bean methyl ester (SBME) was synthesised from raw oil using transesterification
·  SBME and its blends with diesel fuel were investigated for performance, regulated and unregulated emissions
·  B40 blend has lowest smoke, CO, and HC emissions, but highest NOx and CO2 formation 
· B100 blend has lowest toluene and CO2 emissions, but higher acetone emission
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