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· Thermal stability and molecular weight of MMA from RAFT polymerization within the mesoporous materials pore was higher than corresponding polymers from external one due to a confinement effect. 
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PMMA in R-SBA-15 675 132 1574
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