Highlights
· [bookmark: _GoBack]Continuous H2 production from date wastes in CSTR and MBR system
· The maximum H2 production rate (QH2) of 17 mmol/L.h was achieved 
at the dilution rate (D) of 0.25 h-1 in the CSTR
· Increasing D above 0.25 h-1 affected negatively the CSTR performances 
· Integrating membrane with CSTR (MBR) enhanced H2 production rate
· The highest QH2 of 70.2 mmol/L.h was achieved at the D of 0.6 h-1 in the MBR
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