Highlights 
1. Thermal behavior of a new smart internally cooled cutting tool was evaluated
2. Velocity flow and inlet temperature affecting the tip temperature were investigated 
3. The main factor influencing the tip temperatures was found inlet temperature 
4. The percentage contribution ratio of inlet temperature was found to be 88.32
5. Glycol-based fluids can be a better choice for internally cooled cutting tool designs
