Highlights:

Nanocellulose produced from wood by SE pretreatment

A sequential process using SE, phosphorylation and ultra-fine grinding was described 

PMFC and PBMF have a good thermal stability and flame retardancy
