Highlights
• Sustainable process for the intermittently operated MD process was suggested. 
• Scaling and wetting trends in continuous and intermittent operations were compared.
• Shutdown protocols in intermittent mode were evaluated to reduce scaling and wetting.
• Scaling and wetting could be quantified in real-time by using the collected images.
• The collected images in real-time were analyzed by using the normalized intensity.
