Thermal and mechanical abuse of electric vehicle pouch cell modules
Supplementary information
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Figure S1. The location of the thermocouples in the sea container employed in the experiments. Experiment (a) 1, (b) 2 and (c) 3. In experiments 1 and 3 the gas sensors were placed 20 cm, 120 cm and 240 cm from the floor.  In experiment 2 the sensors were placed as shown. Key: Green = H2, blue = NOx, SO2 and CO, purple = HF/HCl. The experiment volumes were defined by the back wall of the container and a polyethylene “blast wall” placed (a) 3 m and (b), (c) 6.1 m from the back wall of the container: i.e. defining 25% or 50% of the volume, respectively, of the 12.2 m x 2.4 m x 2.6 m sea container.
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Figure S2. (a) The 8-cell module, (b) a pouch cell and (c) order of the cell pairs.
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