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Supplementary Figure 1. Level 3 warning interface takeover time under different warnings

	
	First fixation duration within AOI
	P

	level 1
	586 (327.5–891.5)
	＜0.001

	[bookmark: OLE_LINK10]level 2
	267.5 (182.25–423.5)
	

	level 3
	368.5 (271–545.75)
	


[bookmark: OLE_LINK1]Supplementary Table 1. Comparison of the first fixation duration in AOI under different warning levels

	Sample 1 and Sample 2
	Adjusted significance

	level 2 and level 1
	0.118

	level 2 and level 3
	＜0.001

	level 1 and level 3
	0.037


Supplementary Table 2. Pairwise comparison of the significance of the first fixation duration within the AOI under different levels of warning
	
	Total fixation duration in AOI
	P

	level 1
	392 (322.75–527.5)
	＜0.001

	level 2
	531.5 (422–667.25)
	

	level 3
	600.5 (426.75–854.25)
	


Supplementary Table 3. Comparison of total fixation duration in AOI under different warning levels

	Sample 1 and Sample 2
	Adjusted significance

	level 1 and level 2
	0.025

	level 1 and level 3
	＜0.001

	level 2 and level 3
	0.435


Supplementary Table 4. Pairwise comparison of the total fixation duration within the AOI under different levels of warning

	
	Fixation counts in AOI
	P

	level 1
	2 (1–2.33)
	0.001

	level 2
	2 (2–3)
	

	level 3
	1.67 (1.33–2)
	


Supplementary Table 5. Comparison of the fixation count points in AOI under different warning levels

	Sample 1 and Sample 2
	Adjusted significance

	level 1 and level 2 
	1.000

	level 1 and level 3
	0.002

	level 2 and level 3
	0.006


[bookmark: _GoBack]Supplementary Table 6. Pairwise comparison of the significance of the fixation count in the AOI under different levels of warning
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Supplementary Figure 2. Number of eye saccades for level 3 warning interface under different warnings
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Supplementary Figure 3. Maximum saccade velocity of level 3 warning interface under different warnings
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Supplementary Figure 4. Average saccades amplitude of level 3 warning interface under different warnings
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Supplementary Figure 5 Maximum saccades of level 3 warning interface under different warnings
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Supplementary Figure 6. First saccade duration of the level 3 warning interface under different warnings
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