{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Sheet1","Sheet2","Performance","Fuel consump"],"not_rendered":{"charts":16,"external_links":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":8,"rows_kept":20,"merged":[[0,2,1,4]],"flags":["formulas_cached_only"]}
[null,null,"Average Composition of Exhaust Gaseous "]
[]
["S.No","Pure Diesel","5 Percent H2O2","% age reduction","10 Percent H2O2","% age reduction","15 Percent H2O2","% age reduction"]
["Initial temperature T Ambient",25,28,-12,27.75,-11,26,-4]
["Final Temperature T gas",73.5,71.7,2.4489795918367308,63.1,14.149659863945576,78.5,-6.802721088435375]
["Tg-Ta",48.5,43.75,9.793814432989691,35.5,26.804123711340207,52.5,-8.24742268041237]
["CO  (ppm)",565,437.5,22.566371681415927,348.5,38.318584070796454,368,34.86725663716814]
["SO2 (ppm)",16,11,31.25,13.4,16.249999999999996,14.35,10.312500000000002]
["O2  %",19.25,19.25,0,19.5,-1.2987012987012987,19.35,-0.5194805194805269]
["NO2 (ppm)",12,9,25,5.8,51.66666666666667,7.8,35]
["NO (ppm)",3.25,6.15,-89.23076923076924,2,38.46153846153847,1.86,42.76923076923077]
["CxHy %",0.1,0,100,0.07,30,0.05,50]
["H2S (ppm)",0,0.233,null,0,null,0.02]
["CO2 %",1.2,1.75,-45.833333333333336,0.95,20.833333333333336,1.1,8.333333333333323]
["NOx (ppm)",11.5,15.25,-32.608695652173914,7.8,32.173913043478265,9.75,15.217391304347828]
["Efficiency%",67.5,69,-2.2222222222222223,68,-0.7407407407407408,62,8.148148148148149]
["Loss%",32.5,31,4.615384615384616,32,1.5384615384615385,38,-16.923076923076923]
["Excess Air%",1058,1016.25,3.9461247637051042,1137,-7.466918714555766,1093.6,-3.3648393194706907]
["Water %",0,0,null,0,null,0]
["O2 norm %",0,0,null,0,null,0]

{"sheet":"Sheet2","index":1,"n_rows":39,"n_cols":27,"rows_kept":39,"merged":[[3,3,4,4],[3,17,3,20],[32,9,32,11],[32,13,32,15],[33,3,33,4],[33,5,33,6],[33,9,33,11],[33,13,33,15],[33,17,33,18],[33,22,33,23],[33,25,33,26]],"flags":["formulas_cached_only"]}
[]
[]
[]
[{"$nulls":3},"Average Composition of Exhaust Gaseous ",{"$nulls":13},"Unloaded "]
[{"$nulls":17},"RD","5 wt.%","10 wt%","15 wt.%"]
[null,"S.No","Pure Diesel","5 Percent H2O2","10 Percent H2O2","15 Percent H2O2",{"$nulls":10},"TA",25,28,27.75,26]
[null,"Initial temperature T Ambient",25,28,27.75,26,{"$nulls":10},"TG"]
[null,"Final Temperature T gas",73.5,71.7,63.1,78.5,{"$nulls":10},"CxHy %"]
[null,"Tg-Ta",48.5,43.75,35.5,52.5,{"$nulls":10},"O2  %"]
[null,"CO  (ppm)",565,437.5,348.5,368,{"$nulls":10},"Excess Air%"]
[null,"SO2 (ppm)",16,11,13.4,14.35]
[null,"O2  %",19.25,19.25,19.5,19.35]
[null,"NO2 (ppm)",12,9,5.8,7.8]
[null,"NO (ppm)",3.25,6.15,2,1.86]
[null,"CxHy %",0.1,0,0.07,0.05]
[null,"H2S (ppm)",0,0.233,0,0.02]
[null,"CO2 %",1.2,1.75,0.95,1.1]
[null,"NOx (ppm)",11.5,15.25,7.8,9.75]
[null,"Efficiency%",67.5,69,68,62]
[null,"Loss%",32.5,31,32,38]
[null,"Excess Air%",1058,1016.25,1137,1093.6]
[null,"Water %",0,0,0,0]
[null,"O2 norm %",0,0,0,0]
[]
[]
[null,null,"Initial temperature T Ambient","Final Temperature T gas","Tg-Ta","CO  (ppm)","SO2 (ppm)","O2  %","NO2 (ppm)","NO (ppm)","CxHy %","H2S (ppm)","CO2 %","NOx (ppm)"]
[null,"Pure Diesel",25,73.5,48.5,565,16,19.25,12,3.25,0.1,0,1.2,11.5]
[null,"5 Percent H2O2",28,71.7,43.7,437.5,11,19.25,9,6.15,0,0.001,1.75,15.25]
[null,"10 Percent H2O2",27.75,63.1,35.35,348.5,13.4,19.5,5.8,2,0.07,0,0.95,7.8]
[null,"15 Percent H2O2",26,78.5,52.5,368,14.35,19.35,7.8,1.86,0.02,0.009,1.1,9.75]
[]
[]
[{"$nulls":9},"Unloaded",{"$nulls":3},"Loaded"]
[{"$nulls":3},"Unloaded (UL)",null,"Full loaded (FL)",{"$nulls":3},"ppm",{"$nulls":3},"ppm",{"$nulls":3},"ppm",null,null,"%",null,"ET (℃)",null,null,"Air Intake (%)"]
[{"$nulls":3},"CO  (ppm)","CO2 %",{"$nulls":4},"NO2 (UL)","NO (UL)","NOx (UL)",null,"NO2 (FL)","NO (FL)","NOx (FL)",null,"SO2 (UL)","SO2 (FL)",null,"CxHy (UL)","CxHy (FL)","ET-UL","ET-FL",null,"AI-UL","AI-FL"]
[null,"5 Percent H2O2",{"v":0,"d":"0%"},565,1.2,706.25,1.56,null,null,12,3.25,11.5,null,15,4.56,14.37,null,16,20,null,0.1,0.2,73.5,141.12,null,1058,1175.4]
[null,"10 Percent H2O2",{"v":0.05,"d":"5%"},437.5,1.75,525.4,2.1,null,null,9,6.15,15.25,null,10.8,7.38,18.3,null,11,13.2,null,0,0.0001,71.7,112.12,null,1016.25,1067]
[null,"15 Percent H2O2",{"v":0.1,"d":"10%"},348.5,0.95,400.77,1.09,null,null,5.8,2,7.8,null,6.67,2.89,8.9,null,13.4,15.2,null,0.07,0.08,63.1,83.12,null,1037,112.7]
[null,null,{"v":0.15,"d":"15%"},368,1.1,412.16,1.23,null,null,7.8,1.86,9.75,null,8.73,2.08,10.92,null,14.35,16.07,null,0.05,0.07,78.5,85.7,null,1093.6,126.7]

{"sheet":"Performance","index":2,"n_rows":28,"n_cols":13,"rows_kept":28,"flags":["formulas_cached_only"]}
{"$rows_empty":11}
[{"$nulls":3},"CO  (ppm)"]
[]
[]
[]
[]
[{"$nulls":5},"S.No","Pure Diesel","5% H2O2","% age reduction","10% H2O2","% age reduction","15% H2O2","% age reduction"]
[{"$nulls":5},"Initial temperature T Ambient",25,28,-12,27.75,-11,26,-4]
[{"$nulls":5},"Final Temperature T gas",73.5,71.7,2.4489795918367308,63.1,14.149659863945576,78.5,-6.802721088435375]
[{"$nulls":5},"Tg-Ta",48.5,43.75,9.793814432989691,35.5,26.804123711340207,52.5,-8.24742268041237]
[{"$nulls":5},"Efficiency% w/o load",67.5,69,-2.2222222222222223,68,-0.7407407407407408,64,5.185185185185185]
[{"$nulls":5},"Engine Temperature T/hr (w/o load)",300,278,7.333333333333333,262.12,12.626666666666663,258.87,13.709999999999997]
[{"$nulls":5},"Efficiency% with full load",63,62.4,0.9523809523809548,62.14,1.3650793650793642,61.75,1.984126984126984]
[{"$nulls":5},"Engine Temperature T/hr (with load)",380]
[{"$nulls":5},"Loss%",32.5,31,4.615384615384616,32,1.5384615384615385,38,-16.923076923076923]
[{"$nulls":5},"Excess Air%",1058,1016.25,3.9461247637051042,1011.31,4.4130434782608745,998.6,5.614366729678637]
[{"$nulls":5},"Water %",0,0,null,0,null,0]
[{"$nulls":5},"O2 norm %",0,0,null,0,null,0]

{"sheet":"Fuel consump","index":3,"n_rows":10,"n_cols":4,"rows_kept":10,"flags":["formulas_cached_only"]}
[]
[]
[null,null,"ml/hr","ml/hr"]
[null,"Amount of H2O2","W/O Load","With Load"]
[null,0,178.95,317.2]
[null,5,180,321.5]
[null,7,185,331.5]
[null,10,187,335]
[null,12,191,338]
[null,15,193.25,348.51]