Table 1. HIR multimetric breakpoints for five hydromorphological state classes
	River type
	Status of SWB
	The width of riverbed
	Altitude type
	Peat cover of the river valley
	Abiotic types
	HIR multimeter limits appropriate to the class

	
	
	
	
	
	
	I
	II
	III
	IV
	V

	H1
	natural and strongly modified
	≤ 30 m
	uplands and mountains
	-
	1-15***
	≥0.824
	≥0.715
	≥0.600
	≥0.485
	<0.485

	H2
	
	
	lowlands
	no
	16-20, 
22, 25
	≥0.761
	≥0.639
	≥0.500
	≥0.375
	<0.375

	H3
	
	
	
	yes
	23, 24, 26
	≥0.725
	≥0.592
	≥0.459
	≥0.326
	<0.326

	H4
	
	> 30 m
	lowlands**
	-
	21****
	≥0.728
	≥0.629
	≥0.530
	≥0.431
	<0.431

	H5
	artifical*
	-
	-
	-
	0
	≥0.513
	≥0.420
	≥0.342
	≥0.253
	<0.253


* - it does not include artificial dam reservoirs for which the river SWB was created
** - also includes 5 SWBs with a riverbed width > 30 m, located on the San River (abiotic types 14 and 15)
*** - excluding 5 SWBs with a riverbed width > 30 m, located on the San River (abiotic types 14 and 15)
**** - also includes other SWBs with a riverbed width > 30 m, representing abiotic types: 14, 15, 19, 24 and located on the rivers: Wisła, Odra, Warta, Narew, San, Noteć and Wieprz

