Highlights:
· Maximum activity of cellulase is at pH 6.0 and 50°C.
· Optimized enzyme dose is 300 g/t (0.05 IU/g) and reaction time is 90 min.
· Enzymatic deinking removed higher ink (79.3%) than chemical deinking (75.7%).
· Better optical and strength properties were obtained after enzymatic deinking.
· Cellulase assisted deinking of MOW papers is better than chemical deinking.
